SYSTEM system_0
{
   System_Wizard_Version = "5.10";
   System_Wizard_Build = "216";
   WIZARD_SCRIPT_ARGUMENTS 
   {
      device_family = "CYCLONE";
      clock_freq = "100000000";
      generate_hdl = "1";
      generate_sdk = "0";
      do_build_sim = "0";
      hardcopy_compatible = "0";
      board_class = "DE2_Board";
      CLOCKS 
      {
         CLOCK clk
         {
            frequency = "100000000";
            source = "External";
            Is_Clock_Source = "0";
            display_name = "clk";
            pipeline = "0";
            BOARD_COMPONENT altera_nios_dev_board_cyclone_1c20
            {
               pin_assignment = "";
               component_pin = "";
            }
            BOARD_COMPONENT de2_board
            {
               pin_assignment = "";
               component_pin = "use_quartus_pin_assignment";
            }
            BOARD_COMPONENT altera_nios_dev_board_cyclone_2c35
            {
               pin_assignment = "";
               component_pin = "";
            }
         }
      }
      hdl_language = "verilog";
      device_family_id = "CYCLONEII";
      view_master_columns = "1";
      view_master_priorities = "0";
      name_column_width = "363";
      desc_column_width = "363";
      bustype_column_width = "0";
      base_column_width = "75";
      clock_column_width = "80";
      end_column_width = "75";
      view_frame_window = "maximized";
      do_log_history = "0";
      RESETS 
      {
         RESET reset_n
         {
            BOARD_COMPONENT altera_nios_dev_board_cyclone_1c20
            {
               pin_assignment = "";
               component_pin = "use_quartus_pin_assignment";
            }
            BOARD_COMPONENT de2_board
            {
               pin_assignment = "";
               component_pin = "use_quartus_pin_assignment";
            }
            BOARD_COMPONENT altera_nios_dev_board_cyclone_2c35
            {
               pin_assignment = "";
               component_pin = "";
            }
         }
      }
      BOARD_INFO 
      {
         CONFIGURATION EPSC16
         {
            length = "";
            menu_position = "1";
            offset = "0x00000000";
            reference_designator = "U30";
         }
         CONFIGURATION FLASH
         {
            length = "";
            menu_position = "2";
            offset = "0x00000000";
            reference_designator = "U20";
         }
         JTAG_device_index = "1";
         REFDES U20
         {
            base = "0x00400000";
         }
         REFDES U30
         {
            base = "0x00060000";
         }
         altera_avalon_cfi_flash 
         {
            reference_designators = "U20";
         }
         altera_avalon_epcs_flash_controller 
         {
            reference_designators = "U30";
         }
         class = "DE2_Board";
         class_version = "1.0";
         device_family = "CYCLONEII";
         quartus_pgm_file = "system/DE2_Board.sof";
         quartus_project_file = "system/DE2_Board.qpf";
         reference_designators = "U30,U20";
         sopc_system_file = "system/DE2_Board.ptf";
      }
   }
   MODULE cpu_0
   {
      class = "altera_nios2";
      class_version = "5.11";
      iss_model_name = "altera_nios2";
      HDL_INFO 
      {
         PLI_Files = "";
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/cpu_0_test_bench.v, __PROJECT_DIRECTORY__/cpu_0_mult_cell.v, __PROJECT_DIRECTORY__/cpu_0_jtag_debug_module.v, __PROJECT_DIRECTORY__/cpu_0_jtag_debug_module_wrapper.v, __PROJECT_DIRECTORY__/cpu_0.v";
         Synthesis_Only_Files = "";
      }
      MASTER instruction_master
      {
         PORT_WIRING 
         {
            PORT i_address
            {
               Is_Enabled = "1";
               direction = "output";
               type = "address";
               width = "24";
            }
            PORT i_read
            {
               Is_Enabled = "1";
               direction = "output";
               type = "read";
               width = "1";
            }
            PORT i_readdata
            {
               Is_Enabled = "1";
               direction = "input";
               type = "readdata";
               width = "32";
            }
            PORT i_readdatavalid
            {
               Is_Enabled = "1";
               direction = "input";
               type = "readdatavalid";
               width = "1";
            }
            PORT i_waitrequest
            {
               Is_Enabled = "1";
               direction = "input";
               type = "waitrequest";
               width = "1";
            }
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Address_Group = "0";
            Has_IRQ = "0";
            Irq_Scheme = "individual_requests";
            Interrupt_Range = "0-0";
            Is_Enabled = "1";
            Maximum_Burst_Size = "1";
            Burst_On_Burst_Boundaries_Only = "";
            Linewrap_Bursts = "";
            Interleave_Bursts = "";
            Adapts_To = "";
         }
      }
      MASTER tightly_coupled_instruction_master_0
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Instruction_Master = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_1
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_3
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER data_master
      {
         PORT_WIRING 
         {
            PORT clk
            {
               Is_Enabled = "0";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT d_address
            {
               Is_Enabled = "1";
               direction = "output";
               type = "address";
               width = "24";
            }
            PORT d_byteenable
            {
               Is_Enabled = "1";
               direction = "output";
               type = "byteenable";
               width = "4";
            }
            PORT d_irq
            {
               Is_Enabled = "1";
               direction = "input";
               type = "irq";
               width = "32";
            }
            PORT d_read
            {
               Is_Enabled = "1";
               direction = "output";
               type = "read";
               width = "1";
            }
            PORT d_readdata
            {
               Is_Enabled = "1";
               direction = "input";
               type = "readdata";
               width = "32";
            }
            PORT d_waitrequest
            {
               Is_Enabled = "1";
               direction = "input";
               type = "waitrequest";
               width = "1";
            }
            PORT d_write
            {
               Is_Enabled = "1";
               direction = "output";
               type = "write";
               width = "1";
            }
            PORT d_writedata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "writedata";
               width = "32";
            }
            PORT jtag_debug_module_debugaccess_to_roms
            {
               Is_Enabled = "1";
               direction = "output";
               type = "debugaccess";
               width = "1";
            }
            PORT d_readdatavalid
            {
               Is_Enabled = "0";
               direction = "input";
               type = "readdatavalid";
               width = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "1";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "1";
            Irq_Scheme = "individual_requests";
            Interrupt_Range = "0-31";
            Is_Enabled = "1";
            Maximum_Burst_Size = "1";
            Burst_On_Burst_Boundaries_Only = "";
            Adapts_To = "";
         }
      }
      MASTER data_master2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "1";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
         }
      }
      MASTER tightly_coupled_data_master_0
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_data_master_1
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_data_master_2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_data_master_3
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Data_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER custom_instruction_master
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "nios_custom_instruction";
            Data_Width = "32";
            Address_Width = "8";
            Max_Address_Width = "8";
            Base_Address = "N/A";
            Is_Visible = "0";
            Is_Custom_Instruction = "0";
            Is_Enabled = "0";
         }
      }
      SLAVE jtag_debug_module
      {
         PORT_WIRING 
         {
            PORT jtag_debug_module_address
            {
               Is_Enabled = "1";
               direction = "input";
               type = "address";
               width = "9";
            }
            PORT jtag_debug_module_begintransfer
            {
               Is_Enabled = "1";
               direction = "input";
               type = "begintransfer";
               width = "1";
            }
            PORT jtag_debug_module_byteenable
            {
               Is_Enabled = "1";
               direction = "input";
               type = "byteenable";
               width = "4";
            }
            PORT jtag_debug_module_clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT jtag_debug_module_debugaccess
            {
               Is_Enabled = "1";
               direction = "input";
               type = "debugaccess";
               width = "1";
            }
            PORT jtag_debug_module_readdata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readdata";
               width = "32";
            }
            PORT jtag_debug_module_reset
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset";
               width = "1";
            }
            PORT jtag_debug_module_resetrequest
            {
               Is_Enabled = "1";
               direction = "output";
               type = "resetrequest";
               width = "1";
            }
            PORT jtag_debug_module_select
            {
               Is_Enabled = "1";
               direction = "input";
               type = "chipselect";
               width = "1";
            }
            PORT jtag_debug_module_write
            {
               Is_Enabled = "1";
               direction = "input";
               type = "write";
               width = "1";
            }
            PORT jtag_debug_module_writedata
            {
               Is_Enabled = "1";
               direction = "input";
               type = "writedata";
               width = "32";
            }
            PORT reset_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset_n";
               width = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Read_Wait_States = "1";
            Write_Wait_States = "1";
            Register_Incoming_Signals = "1";
            Bus_Type = "avalon";
            Data_Width = "32";
            Address_Width = "9";
            Accepts_Internal_Connections = "1";
            Requires_Internal_Connections = "instruction_master,data_master";
            Accepts_External_Connections = "0";
            Is_Enabled = "1";
            Address_Alignment = "dynamic";
            Base_Address = "0x00480000";
            Is_Memory_Device = "1";
            Is_Readable = "1";
            Is_Writeable = "1";
            Is_Printable_Device = "0";
            Uses_Tri_State_Data_Bus = "0";
            Has_IRQ = "0";
            JTAG_Hub_Base_Id = "1118278";
            JTAG_Hub_Instance_Id = "0";
            MASTERED_BY cpu_0/instruction_master
            {
               priority = "1";
            }
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Address_Group = "0";
         }
      }
      PORT_WIRING 
      {
         PORT jtag_debug_trigout
         {
            width = "1";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT jtag_debug_offchip_trace_clk
         {
            width = "1";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT jtag_debug_offchip_trace_data
         {
            width = "18";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT clkx2
         {
            width = "1";
            direction = "input";
            Is_Enabled = "0";
            visible = "0";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         asp_debug = "0";
         asp_core_debug = "0";
         CPU_Architecture = "nios2";
         do_generate = "1";
         cpu_selection = "f";
         CPU_Implementation = "fast";
         gui_include_tightly_coupled_instruction_masters = "0";
         gui_num_tightly_coupled_instruction_masters = "1";
         gui_omit_avalon_data_master = "0";
         gui_include_tightly_coupled_data_masters = "0";
         gui_num_tightly_coupled_data_masters = "1";
         num_tightly_coupled_instruction_masters = "0";
         num_tightly_coupled_data_masters = "0";
         cache_has_dcache = "1";
         cache_has_icache = "1";
         cache_dcache_size = "16384";
         cache_icache_size = "16384";
         cache_dcache_line_size = "4";
         cache_icache_line_size = "32";
         cache_dcache_bursts = "0";
         cache_icache_burst_type = "none";
         cache_dcache_ram_block_type = "AUTO";
         cache_icache_ram_block_type = "AUTO";
         include_debug = "0";
         include_trace = "0";
         include_oci = "1";
         include_third_party_debug_port = "0";
         debug_level = "2";
         oci_offchip_trace = "0";
         oci_onchip_trace = "0";
         oci_data_trace = "0";
         oci_trace_addr_width = "7";
         oci_num_xbrk = "0";
         oci_num_dbrk = "0";
         oci_dbrk_trace = "0";
         oci_dbrk_pairs = "0";
         oci_num_pm = "0";
         oci_pm_width = "40";
         oci_debugreq_signals = "0";
         oci_trigger_arming = "1";
         oci_embedded_pll = "1";
         hardware_multiply_present = "1";
         hardware_divide_present = "1";
         gui_hardware_multiply_setting = "embedded_mul_fast_le_shift";
         hardware_multiply_uses_les = "0";
         hardware_multiply_omits_msw = "1";
         hardware_multiply_impl = "embedded_mul";
         gui_hardware_divide_setting = "1";
         reset_slave = "epcs_controller/epcs_control_port";
         reset_offset = "0x00000000";
         exc_slave = "sdram_0/s1";
         exc_offset = "0x00000020";
         break_slave = "cpu_0/jtag_debug_module";
         break_offset = "0x00000020";
         break_slave_override = "";
         break_offset_override = "0x20";
         legacy_sdk_support = "0";
         altera_show_unreleased_features = "0";
         full_waveform_signals = "0";
         illegal_instructions_trap = "0";
         gui_branch_prediction_type = "Automatic";
         branch_prediction_type = "Dynamic";
         bht_ptr_sz = "8";
         bht_index_pc_only = "0";
         shift_rot_impl = "fast_le_shift";
         mmu_present = "0";
         process_id_num_bits = "10";
         dtlb_ptr_sz = "7";
         dtlb_num_ways = "4";
         udtlb_num_entries = "6";
         itlb_ptr_sz = "7";
         itlb_num_ways = "4";
         uitlb_num_entries = "4";
         fast_tlb_miss_exc_slave = "";
         fast_tlb_miss_exc_offset = "0x0";
         cache_omit_dcache = "0";
         cache_omit_icache = "0";
         omit_instruction_master = "0";
         omit_data_master = "0";
         altera_internal_test = "0";
         performance_counters_present = "0";
         performance_counters_width = "32";
         ras_ptr_sz = "4";
         jtb_ptr_sz = "5";
         ibuf_ptr_sz = "4";
         always_encrypt = "1";
         activate_model_checker = "0";
         activate_monitors = "1";
         activate_test_end_checker = "0";
         activate_trace = "1";
         clear_x_bits_ld_non_bypass = "1";
         bit_31_bypass_dcache = "1";
         always_bypass_dcache = "0";
         hdl_sim_caches_cleared = "1";
         consistent_synthesis = "0";
         hbreak_test = "0";
         allow_full_address_range = "0";
         iss_trace_on = "0";
         iss_trace_warning = "1";
         iss_trace_info = "1";
         iss_trace_disassembly = "0";
         iss_trace_registers = "0";
         iss_trace_instr_count = "0";
         iss_software_debug = "0";
         iss_software_debug_port = "9996";
         iss_memory_dump_start = "";
         iss_memory_dump_end = "";
         Boot_Copier = "boot_loader_cfi.srec";
         Boot_Copier_EPCS = "boot_loader_epcs.srec";
         CONSTANTS 
         {
            CONSTANT __nios_catch_irqs__
            {
               value = "1";
               comment = "Include panic handler for all irqs (needs uart)";
            }
            CONSTANT __nios_use_constructors__
            {
               value = "1";
               comment = "Call c++ static constructors";
            }
            CONSTANT __nios_use_small_printf__
            {
               value = "1";
               comment = "Smaller non-ANSI printf, with no floating point";
            }
            CONSTANT nasys_has_icache
            {
               value = "1";
               comment = "True if instruction cache present";
            }
            CONSTANT nasys_icache_size
            {
               value = "16384";
               comment = "Size in bytes of instruction cache";
            }
            CONSTANT nasys_icache_line_size
            {
               value = "32";
               comment = "Size in bytes of each icache line";
            }
            CONSTANT nasys_icache_line_size_log2
            {
               value = "5";
               comment = "Log2 size in bytes of each icache line";
            }
            CONSTANT nasys_has_dcache
            {
               value = "1";
               comment = "True if instruction cache present";
            }
            CONSTANT nasys_dcache_size
            {
               value = "16384";
               comment = "Size in bytes of data cache";
            }
            CONSTANT nasys_dcache_line_size
            {
               value = "4";
               comment = "Size in bytes of each dcache line";
            }
            CONSTANT nasys_dcache_line_size_log2
            {
               value = "2";
               comment = "Log2 size in bytes of each dcache line";
            }
         }
         license_status = "encrypted";
         germs_monitor_id = "";
         cpuid_sz = "1";
         cpuid_value = "0";
         gui_illegal_instructions_trap = "0";
         gui_illegal_memory_access_detection = "0";
         illegal_memory_access_detection = "0";
         gui_mmu_present = "0";
         debug_simgen = "0";
      }
      SYSTEM_BUILDER_INFO 
      {
         Parameters_Signature = "";
         Is_CPU = "1";
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Required_Device_Family = "STRATIX,STRATIXGX,STRATIXII,STRATIXIIGX,CYCLONE,CYCLONEII";
         Default_Module_Name = "cpu";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            MESSAGES 
            {
            }
            Is_Collapsed = "0";
            Settings_Summary = "Nios II/f
            <br>&nbsp;&nbsp;16-Kbyte Instruction Cache
            <br>&nbsp;&nbsp;16-Kbyte Data Cache
            <br>&nbsp;&nbsp;JTAG Debug Module
            ";
         }
      }
      SOFTWARE_COMPONENT altera_plugs_library
      {
         class = "altera_plugs_library";
         class_version = "2.1";
         WIZARD_SCRIPT_ARGUMENTS 
         {
            CONSTANTS 
            {
               CONSTANT PLUGS_PLUG_COUNT
               {
                  value = "5";
                  comment = "Maximum number of plugs";
               }
               CONSTANT PLUGS_ADAPTER_COUNT
               {
                  value = "2";
                  comment = "Maximum number of adapters";
               }
               CONSTANT PLUGS_DNS
               {
                  value = "1";
                  comment = "Have routines for DNS lookups";
               }
               CONSTANT PLUGS_PING
               {
                  value = "1";
                  comment = "Respond to icmp echo (ping) messages";
               }
               CONSTANT PLUGS_TCP
               {
                  value = "1";
                  comment = "Support tcp in/out connections";
               }
               CONSTANT PLUGS_IRQ
               {
                  value = "1";
                  comment = "Run at interrupte level";
               }
               CONSTANT PLUGS_DEBUG
               {
                  value = "1";
                  comment = "Support debug routines";
               }
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Is_Enabled = "1";
         }
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL aaa
            {
               format = "Logic";
               name = "i_readdata";
               radix = "hexadecimal";
            }
            SIGNAL aab
            {
               format = "Logic";
               name = "i_readdatavalid";
               radix = "hexadecimal";
            }
            SIGNAL aac
            {
               format = "Logic";
               name = "i_waitrequest";
               radix = "hexadecimal";
            }
            SIGNAL aad
            {
               format = "Logic";
               name = "i_address";
               radix = "hexadecimal";
            }
            SIGNAL aae
            {
               format = "Logic";
               name = "i_read";
               radix = "hexadecimal";
            }
            SIGNAL aaf
            {
               format = "Logic";
               name = "clk";
               radix = "hexadecimal";
            }
            SIGNAL aag
            {
               format = "Logic";
               name = "reset_n";
               radix = "hexadecimal";
            }
            SIGNAL aah
            {
               format = "Logic";
               name = "d_readdata";
               radix = "hexadecimal";
            }
            SIGNAL aai
            {
               format = "Logic";
               name = "d_waitrequest";
               radix = "hexadecimal";
            }
            SIGNAL aaj
            {
               format = "Logic";
               name = "d_irq";
               radix = "hexadecimal";
            }
            SIGNAL aak
            {
               format = "Logic";
               name = "d_address";
               radix = "hexadecimal";
            }
            SIGNAL aal
            {
               format = "Logic";
               name = "d_byteenable";
               radix = "hexadecimal";
            }
            SIGNAL aam
            {
               format = "Logic";
               name = "d_read";
               radix = "hexadecimal";
            }
            SIGNAL aan
            {
               format = "Logic";
               name = "d_write";
               radix = "hexadecimal";
            }
            SIGNAL aao
            {
               format = "Logic";
               name = "d_writedata";
               radix = "hexadecimal";
            }
            SIGNAL aap
            {
               format = "Divider";
               name = "base pipeline";
               radix = "";
            }
            SIGNAL aaq
            {
               format = "Logic";
               name = "clk";
               radix = "hexadecimal";
            }
            SIGNAL aar
            {
               format = "Logic";
               name = "reset_n";
               radix = "hexadecimal";
            }
            SIGNAL aas
            {
               format = "Logic";
               name = "D_stall";
               radix = "hexadecimal";
            }
            SIGNAL aat
            {
               format = "Logic";
               name = "A_stall";
               radix = "hexadecimal";
            }
            SIGNAL aau
            {
               format = "Logic";
               name = "F_pcb_nxt";
               radix = "hexadecimal";
            }
            SIGNAL aav
            {
               format = "Logic";
               name = "F_pcb";
               radix = "hexadecimal";
            }
            SIGNAL aaw
            {
               format = "Logic";
               name = "D_pcb";
               radix = "hexadecimal";
            }
            SIGNAL aax
            {
               format = "Logic";
               name = "E_pcb";
               radix = "hexadecimal";
            }
            SIGNAL aay
            {
               format = "Logic";
               name = "M_pcb";
               radix = "hexadecimal";
            }
            SIGNAL aaz
            {
               format = "Logic";
               name = "A_pcb";
               radix = "hexadecimal";
            }
            SIGNAL aba
            {
               format = "Logic";
               name = "W_pcb";
               radix = "hexadecimal";
            }
            SIGNAL abb
            {
               format = "Logic";
               name = "F_vinst";
               radix = "ascii";
            }
            SIGNAL abc
            {
               format = "Logic";
               name = "D_vinst";
               radix = "ascii";
            }
            SIGNAL abd
            {
               format = "Logic";
               name = "E_vinst";
               radix = "ascii";
            }
            SIGNAL abe
            {
               format = "Logic";
               name = "M_vinst";
               radix = "ascii";
            }
            SIGNAL abf
            {
               format = "Logic";
               name = "A_vinst";
               radix = "ascii";
            }
            SIGNAL abg
            {
               format = "Logic";
               name = "W_vinst";
               radix = "ascii";
            }
            SIGNAL abh
            {
               format = "Logic";
               name = "F_inst_ram_hit";
               radix = "hexadecimal";
            }
            SIGNAL abi
            {
               format = "Logic";
               name = "F_issue";
               radix = "hexadecimal";
            }
            SIGNAL abj
            {
               format = "Logic";
               name = "F_kill";
               radix = "hexadecimal";
            }
            SIGNAL abk
            {
               format = "Logic";
               name = "D_kill";
               radix = "hexadecimal";
            }
            SIGNAL abl
            {
               format = "Logic";
               name = "D_refetch";
               radix = "hexadecimal";
            }
            SIGNAL abm
            {
               format = "Logic";
               name = "D_issue";
               radix = "hexadecimal";
            }
            SIGNAL abn
            {
               format = "Logic";
               name = "D_valid";
               radix = "hexadecimal";
            }
            SIGNAL abo
            {
               format = "Logic";
               name = "E_valid";
               radix = "hexadecimal";
            }
            SIGNAL abp
            {
               format = "Logic";
               name = "M_valid";
               radix = "hexadecimal";
            }
            SIGNAL abq
            {
               format = "Logic";
               name = "A_valid";
               radix = "hexadecimal";
            }
            SIGNAL abr
            {
               format = "Logic";
               name = "W_valid";
               radix = "hexadecimal";
            }
            SIGNAL abs
            {
               format = "Logic";
               name = "W_wr_dst_reg";
               radix = "hexadecimal";
            }
            SIGNAL abt
            {
               format = "Logic";
               name = "W_dst_regnum";
               radix = "hexadecimal";
            }
            SIGNAL abu
            {
               format = "Logic";
               name = "W_wr_data";
               radix = "hexadecimal";
            }
            SIGNAL abv
            {
               format = "Logic";
               name = "D_en";
               radix = "hexadecimal";
            }
            SIGNAL abw
            {
               format = "Logic";
               name = "E_en";
               radix = "hexadecimal";
            }
            SIGNAL abx
            {
               format = "Logic";
               name = "M_en";
               radix = "hexadecimal";
            }
            SIGNAL aby
            {
               format = "Logic";
               name = "A_en";
               radix = "hexadecimal";
            }
            SIGNAL abz
            {
               format = "Logic";
               name = "F_iw";
               radix = "hexadecimal";
            }
            SIGNAL aca
            {
               format = "Logic";
               name = "D_iw";
               radix = "hexadecimal";
            }
            SIGNAL acb
            {
               format = "Logic";
               name = "E_iw";
               radix = "hexadecimal";
            }
            SIGNAL acc
            {
               format = "Logic";
               name = "E_valid_prior_to_hbreak";
               radix = "hexadecimal";
            }
            SIGNAL acd
            {
               format = "Logic";
               name = "M_pipe_flush";
               radix = "hexadecimal";
            }
            SIGNAL ace
            {
               format = "Logic";
               name = "M_pipe_flush_baddr";
               radix = "hexadecimal";
            }
            SIGNAL acf
            {
               format = "Logic";
               name = "intr_req";
               radix = "hexadecimal";
            }
            SIGNAL acg
            {
               format = "Logic";
               name = "A_ienable_reg";
               radix = "hexadecimal";
            }
            SIGNAL ach
            {
               format = "Logic";
               name = "A_status_reg_pie";
               radix = "hexadecimal";
            }
            SIGNAL aci
            {
               format = "Logic";
               name = "E_valid_prior_to_hbreak";
               radix = "hexadecimal";
            }
         }
      }
   }
   MODULE tri_state_bridge_0
   {
      class = "altera_avalon_tri_state_bridge";
      class_version = "5.11";
      SLAVE avalon_slave
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Bridges_To = "tristate_master";
            Base_Address = "N/A";
            Has_IRQ = "0";
            IRQ = "N/A";
            Register_Outgoing_Signals = "1";
            Register_Incoming_Signals = "1";
            MASTERED_BY cpu_0/instruction_master
            {
               priority = "1";
            }
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Address_Group = "0";
         }
      }
      MASTER tristate_master
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon_tristate";
            Bridges_To = "avalon_slave";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Is_Bridge = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
      }
   }
   MODULE cfi_flash_0
   {
      class = "altera_avalon_cfi_flash";
      class_version = "5.11";
      iss_model_name = "altera_avalon_flash";
      HDL_INFO 
      {
      }
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT data
            {
               width = "8";
               is_shared = "1";
               direction = "inout";
               type = "data";
               originally_shared = "1";
            }
            PORT address
            {
               width = "22";
               is_shared = "1";
               direction = "input";
               type = "address";
               originally_shared = "1";
            }
            PORT read_n
            {
               width = "1";
               is_shared = "1";
               direction = "input";
               type = "read_n";
               originally_shared = "1";
            }
            PORT write_n
            {
               width = "1";
               is_shared = "0";
               direction = "input";
               type = "write_n";
               originally_shared = "0";
            }
            PORT select_n
            {
               width = "1";
               is_shared = "0";
               direction = "input";
               type = "chipselect_n";
               originally_shared = "0";
            }
         }
         WIZARD_SCRIPT_ARGUMENTS 
         {
            class = "altera_avalon_cfi_flash";
            Supports_Flash_File_System = "1";
            flash_reference_designator = "U20";
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon_tristate";
            Is_Nonvolatile_Storage = "1";
            Is_Memory_Device = "1";
            Address_Alignment = "dynamic";
            Has_IRQ = "0";
            Base_Address = "0x00000000";
            Data_Width = "8";
            Address_Width = "22";
            Simulation_Num_Lanes = "1";
            Convert_Xs_To_0 = "1";
            Write_Wait_States = "160ns";
            Read_Wait_States = "160ns";
            Setup_Time = "40ns";
            Hold_Time = "40ns";
            Address_Span = "4194304";
            MASTERED_BY tri_state_bridge_0/tristate_master
            {
               priority = "1";
            }
            Is_Base_Locked = "1";
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Address_Group = "0";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Make_Memory_Model = "1";
         Is_Enabled = "1";
         Instantiate_In_System_Module = "0";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Setup_Value = "40";
         Wait_Value = "160";
         Hold_Value = "40";
         Timing_Units = "ns";
         Unit_Multiplier = "1";
         Size = "4194304";
         MAKE 
         {
            MACRO 
            {
               CFI_FLASH_0_FLASHTARGET_ALT_SIM_PREFIX = "$(CFI_FLASH_0_FLASHTARGET_TMP1:0=)";
               CFI_FLASH_0_FLASHTARGET_TMP1 = "$(ALT_SIM_OPTIMIZE:1=RUN_ON_HDL_SIMULATOR_ONLY_)";
            }
            MASTER cpu_0
            {
               MACRO 
               {
                  BOOT_COPIER = "boot_loader_cfi.srec";
                  CPU_CLASS = "altera_nios2";
                  CPU_RESET_ADDRESS = "0x480800";
               }
            }
            TARGET delete_placeholder_warning
            {
               cfi_flash_0 
               {
                  Command1 = "rm -f $(SIMDIR)/contents_file_warning.txt";
                  Is_Phony = "1";
                  Target_File = "do_delete_placeholder_warning";
               }
            }
            TARGET flashfiles
            {
               cfi_flash_0 
               {
                  Command1 = "@echo Post-processing to create $(notdir $@)";
                  Command2 = "elf2flash --input=$(ELF) --flash=U20 --boot=$(shell $(QUARTUS_ROOTDIR)/sopc_builder/bin/find_sopc_component_dir $(CPU_CLASS) $(QUARTUS_PROJECT_DIR))/$(BOOT_COPIER) --outfile=$(CFI_FLASH_0_FLASHTARGET_ALT_SIM_PREFIX)cfi_flash_0.flash --sim_optimize=$(ALT_SIM_OPTIMIZE) --base=0x0 --end=0x3FFFFF --reset=$(CPU_RESET_ADDRESS) ";
                  Dependency = "$(ELF)";
                  Target_File = "$(CFI_FLASH_0_FLASHTARGET_ALT_SIM_PREFIX)cfi_flash_0.flash";
               }
            }
            TARGET sim
            {
               cfi_flash_0 
               {
                  Command1 = "if [ ! -d $(SIMDIR) ]; then mkdir $(SIMDIR) ; fi";
                  Command2 = "@echo Hardware simulation is not enabled for the target SOPC Builder system. Skipping creation of hardware simulation model contents and simulation symbol files. \\(Note: This does not affect the instruction set simulator.\\)";
                  Command3 = "touch $(SIMDIR)/dummy_file";
                  Dependency = "$(ELF)";
                  Target_File = "$(SIMDIR)/dummy_file";
               }
            }
         }
         contents_info = "SIMDIR/cfi_flash_0.dat 1130817963 ";
      }
   }
   MODULE sdram_0
   {
      class = "altera_avalon_new_sdram_controller";
      class_version = "5.11";
      iss_model_name = "altera_memory";
      SLAVE s1
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Address_Alignment = "dynamic";
            Has_IRQ = "0";
            Maximum_Pending_Read_Transactions = "7";
            Read_Wait_States = "peripheral_controlled";
            Write_Wait_States = "peripheral_controlled";
            Is_Memory_Device = "1";
            Address_Width = "22";
            Data_Width = "16";
            Simulation_Num_Lanes = "1";
            MASTERED_BY cpu_0/instruction_master
            {
               priority = "1";
            }
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            Base_Address = "0x00800000";
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Address_Group = "0";
         }
         PORT_WIRING 
         {
            PORT zs_addr
            {
               direction = "output";
               width = "12";
               Is_Enabled = "1";
               originally_shared = "0";
               is_shared = "0";
            }
            PORT zs_ba
            {
               direction = "output";
               width = "2";
               Is_Enabled = "1";
               originally_shared = "0";
               is_shared = "0";
            }
            PORT zs_cas_n
            {
               direction = "output";
               width = "1";
               Is_Enabled = "1";
               originally_shared = "0";
               is_shared = "0";
            }
            PORT zs_cke
            {
               direction = "output";
               width = "1";
               Is_Enabled = "1";
               originally_shared = "0";
               is_shared = "0";
            }
            PORT zs_cs_n
            {
               direction = "output";
               width = "1";
               Is_Enabled = "1";
               originally_shared = "0";
               is_shared = "0";
            }
            PORT zs_dq
            {
               direction = "inout";
               width = "16";
               Is_Enabled = "1";
               originally_shared = "0";
               is_shared = "0";
            }
            PORT zs_dqm
            {
               direction = "output";
               width = "2";
               Is_Enabled = "1";
               originally_shared = "0";
               is_shared = "0";
            }
            PORT zs_ras_n
            {
               direction = "output";
               width = "1";
               Is_Enabled = "1";
               originally_shared = "0";
               is_shared = "0";
            }
            PORT zs_we_n
            {
               direction = "output";
               width = "1";
               Is_Enabled = "1";
               originally_shared = "0";
               is_shared = "0";
            }
            PORT az_addr
            {
               Is_Enabled = "1";
               direction = "input";
               type = "address";
               width = "22";
            }
            PORT az_be_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "byteenable_n";
               width = "2";
            }
            PORT az_cs
            {
               Is_Enabled = "1";
               direction = "input";
               type = "chipselect";
               width = "1";
            }
            PORT az_data
            {
               Is_Enabled = "1";
               direction = "input";
               type = "writedata";
               width = "16";
            }
            PORT az_rd_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "read_n";
               width = "1";
            }
            PORT az_wr_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "write_n";
               width = "1";
            }
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT reset_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset_n";
               width = "1";
            }
            PORT za_data
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readdata";
               width = "16";
            }
            PORT za_valid
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readdatavalid";
               width = "1";
            }
            PORT za_waitrequest
            {
               Is_Enabled = "1";
               direction = "output";
               type = "waitrequest";
               width = "1";
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Default_Module_Name = "sdram";
         Disable_Simulation_Port_Wiring = "0";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            Settings_Summary = "4194304 x 16<br>
                Memory size: 8 MBytes<br>
                64 MBits
                ";
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         register_data_in = "1";
         sim_model_base = "1";
         sdram_data_width = "16";
         sdram_addr_width = "12";
         sdram_row_width = "12";
         sdram_col_width = "8";
         sdram_num_chipselects = "1";
         sdram_num_banks = "4";
         refresh_period = "15.625";
         powerup_delay = "100";
         cas_latency = "3";
         t_rfc = "70";
         t_rp = "20";
         t_mrd = "3";
         t_rcd = "20";
         t_ac = "5.5";
         t_wr = "14";
         init_refresh_commands = "2";
         init_nop_delay = "0";
         shared_data = "0";
         starvation_indicator = "0";
         tristate_bridge_slave = "";
         is_initialized = "1";
         sdram_bank_width = "2";
         MAKE 
         {
            TARGET delete_placeholder_warning
            {
               sdram_0 
               {
                  Command1 = "rm -f $(SIMDIR)/contents_file_warning.txt";
                  Is_Phony = "1";
                  Target_File = "do_delete_placeholder_warning";
               }
            }
            TARGET sim
            {
               sdram_0 
               {
                  Command1 = "if [ ! -d $(SIMDIR) ]; then mkdir $(SIMDIR) ; fi";
                  Command2 = "@echo Hardware simulation is not enabled for the target SOPC Builder system. Skipping creation of hardware simulation model contents and simulation symbol files. \\(Note: This does not affect the instruction set simulator.\\)";
                  Command3 = "touch $(SIMDIR)/dummy_file";
                  Dependency = "$(ELF)";
                  Target_File = "$(SIMDIR)/dummy_file";
               }
            }
         }
         contents_info = "SIMDIR/sdram_0.dat 1130817965 ";
      }
      SIMULATION 
      {
         Fix_Me_Up = "";
         DISPLAY 
         {
            SIGNAL a
            {
               name = "az_addr";
               radix = "hexadecimal";
            }
            SIGNAL b
            {
               name = "az_be_n";
               radix = "hexadecimal";
            }
            SIGNAL c
            {
               name = "az_cs";
            }
            SIGNAL d
            {
               name = "az_data";
               radix = "hexadecimal";
            }
            SIGNAL e
            {
               name = "az_rd_n";
            }
            SIGNAL f
            {
               name = "az_wr_n";
            }
            SIGNAL g
            {
               name = "clk";
            }
            SIGNAL h
            {
               name = "za_data";
               radix = "hexadecimal";
            }
            SIGNAL i
            {
               name = "za_valid";
            }
            SIGNAL j
            {
               name = "za_waitrequest";
            }
            SIGNAL k
            {
               name = "za_cannotrefresh";
               suppress = "1";
            }
            SIGNAL l
            {
               name = "CODE";
               radix = "ascii";
            }
            SIGNAL m
            {
               name = "zs_addr";
               radix = "hexadecimal";
               suppress = "0";
            }
            SIGNAL n
            {
               name = "zs_ba";
               radix = "hexadecimal";
               suppress = "0";
            }
            SIGNAL o
            {
               name = "zs_cs_n";
               radix = "hexadecimal";
               suppress = "0";
            }
            SIGNAL p
            {
               name = "zs_ras_n";
               suppress = "0";
            }
            SIGNAL q
            {
               name = "zs_cas_n";
               suppress = "0";
            }
            SIGNAL r
            {
               name = "zs_we_n";
               suppress = "0";
            }
            SIGNAL s
            {
               name = "zs_dq";
               radix = "hexadecimal";
               suppress = "0";
            }
            SIGNAL t
            {
               name = "zs_dqm";
               radix = "hexadecimal";
               suppress = "0";
            }
            SIGNAL u
            {
               name = "zt_addr";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL v
            {
               name = "zt_ba";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL w
            {
               name = "zt_oe";
               suppress = "1";
            }
            SIGNAL x
            {
               name = "zt_cke";
               suppress = "1";
            }
            SIGNAL y
            {
               name = "zt_chipselect";
               suppress = "1";
            }
            SIGNAL z0
            {
               name = "zt_lock_n";
               suppress = "1";
            }
            SIGNAL z1
            {
               name = "zt_ras_n";
               suppress = "1";
            }
            SIGNAL z2
            {
               name = "zt_cas_n";
               suppress = "1";
            }
            SIGNAL z3
            {
               name = "zt_we_n";
               suppress = "1";
            }
            SIGNAL z4
            {
               name = "zt_cs_n";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL z5
            {
               name = "zt_dqm";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL z6
            {
               name = "zt_data";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL z7
            {
               name = "tz_data";
               radix = "hexadecimal";
               suppress = "1";
            }
            SIGNAL z8
            {
               name = "tz_waitrequest";
               suppress = "1";
            }
         }
         PORT_WIRING 
         {
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               width = "1";
            }
            PORT zs_addr
            {
               Is_Enabled = "1";
               direction = "input";
               width = "12";
            }
            PORT zs_ba
            {
               Is_Enabled = "1";
               direction = "input";
               width = "2";
            }
            PORT zs_cas_n
            {
               Is_Enabled = "1";
               direction = "input";
               width = "1";
            }
            PORT zs_cke
            {
               Is_Enabled = "1";
               direction = "input";
               width = "1";
            }
            PORT zs_cs_n
            {
               Is_Enabled = "1";
               direction = "input";
               width = "1";
            }
            PORT zs_dq
            {
               Is_Enabled = "1";
               direction = "inout";
               width = "16";
            }
            PORT zs_dqm
            {
               Is_Enabled = "1";
               direction = "input";
               width = "2";
            }
            PORT zs_ras_n
            {
               Is_Enabled = "1";
               direction = "input";
               width = "1";
            }
            PORT zs_we_n
            {
               Is_Enabled = "1";
               direction = "input";
               width = "1";
            }
         }
      }
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/sdram_0.v, __PROJECT_DIRECTORY__/sdram_0_test_component.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
      }
   }
   MODULE epcs_controller
   {
      class = "altera_avalon_epcs_flash_controller";
      class_version = "5.1";
      SLAVE epcs_control_port
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Nonvolatile_Storage = "1";
            Is_Printable_Device = "0";
            Address_Alignment = "dynamic";
            Is_Memory_Device = "1";
            Address_Width = "9";
            Data_Width = "32";
            Has_IRQ = "1";
            Read_Wait_States = "1";
            Write_Wait_States = "1";
            MASTERED_BY cpu_0/instruction_master
            {
               priority = "1";
            }
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "0";
            }
            Base_Address = "0x00480800";
            Address_Group = "0";
         }
         WIZARD_SCRIPT_ARGUMENTS 
         {
            class = "altera_avalon_epcs_flash_controller";
            flash_reference_designator = "U30";
         }
         PORT_WIRING 
         {
            PORT address
            {
               Is_Enabled = "1";
               direction = "input";
               type = "address";
               width = "9";
            }
            PORT chipselect
            {
               Is_Enabled = "1";
               direction = "input";
               type = "chipselect";
               width = "1";
            }
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT data_from_cpu
            {
               Is_Enabled = "0";
               direction = "input";
               type = "writedata";
               width = "16";
            }
            PORT data_to_cpu
            {
               Is_Enabled = "0";
               direction = "output";
               type = "readdata";
               width = "16";
            }
            PORT dataavailable
            {
               Is_Enabled = "1";
               direction = "output";
               type = "dataavailable";
               width = "1";
            }
            PORT endofpacket
            {
               Is_Enabled = "1";
               direction = "output";
               type = "endofpacket";
               width = "1";
            }
            PORT epcs_select
            {
               Is_Enabled = "0";
               direction = "input";
               type = "chipselect";
               width = "1";
            }
            PORT irq
            {
               Is_Enabled = "1";
               direction = "output";
               type = "irq";
               width = "1";
            }
            PORT mem_addr
            {
               Is_Enabled = "0";
               direction = "input";
               type = "address";
               width = "3";
            }
            PORT read_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "read_n";
               width = "1";
            }
            PORT readdata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readdata";
               width = "32";
            }
            PORT readyfordata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readyfordata";
               width = "1";
            }
            PORT reset_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset_n";
               width = "1";
            }
            PORT write_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "write_n";
               width = "1";
            }
            PORT writedata
            {
               Is_Enabled = "1";
               direction = "input";
               type = "writedata";
               width = "32";
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Required_Device_Family = "CYCLONE,CYCLONEII,STRATIXII,STRATIXIIGX";
         Fixed_Module_Name = "epcs_controller";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         databits = "8";
         targetclock = "20";
         clockunits = "MHz";
         clockmult = "1000000";
         numslaves = "1";
         ismaster = "1";
         clockpolarity = "0";
         clockphase = "0";
         lsbfirst = "0";
         extradelay = "0";
         targetssdelay = "100";
         delayunits = "us";
         delaymult = "1e-006";
         prefix = "epcs_";
         register_offset = "0x200";
         MAKE 
         {
            MACRO 
            {
               EPCS_CONTROLLER_BOOT_ROM_FLASHTARGET_ALT_SIM_PREFIX = "$(EPCS_CONTROLLER_BOOT_ROM_FLASHTARGET_TMP1:0=)";
               EPCS_CONTROLLER_BOOT_ROM_FLASHTARGET_TMP1 = "$(ALT_SIM_OPTIMIZE:1=RUN_ON_HDL_SIMULATOR_ONLY_)";
            }
            MASTER cpu_0
            {
               MACRO 
               {
                  BOOTS_FROM_EPCS = "1";
                  BOOT_COPIER_EPCS = "boot_loader_epcs.srec";
                  CPU_CLASS = "altera_nios2";
                  CPU_RESET_ADDRESS = "0x480800";
               }
            }
            TARGET delete_placeholder_warning
            {
               epcs_controller 
               {
                  Command1 = "rm -f $(SIMDIR)/contents_file_warning.txt";
                  Is_Phony = "1";
                  Target_File = "do_delete_placeholder_warning";
               }
            }
            TARGET flashfiles
            {
               epcs_controller 
               {
                  Command1 = "@if [ $(BOOTS_FROM_EPCS) -eq 1 ]; then echo Post-processing to create $(notdir $@) ; elf2flash --input=$(ELF) --flash=U30 --boot=$(shell $(QUARTUS_ROOTDIR)/sopc_builder/bin/find_sopc_component_dir $(CPU_CLASS) $(QUARTUS_PROJECT_DIR))/$(BOOT_COPIER_EPCS) --outfile=$(EPCS_CONTROLLER_BOOT_ROM_FLASHTARGET_ALT_SIM_PREFIX)epcs_controller_boot_rom.flash --sim_optimize=$(ALT_SIM_OPTIMIZE) --epcs --base=0x0 --end=0x7FFFFFFF  ; fi";
                  Dependency = "$(ELF)";
                  Target_File = "$(EPCS_CONTROLLER_BOOT_ROM_FLASHTARGET_ALT_SIM_PREFIX)epcs_controller_boot_rom.flash";
               }
            }
            TARGET sim
            {
               epcs_controller 
               {
                  Command1 = "if [ ! -d $(SIMDIR) ]; then mkdir $(SIMDIR) ; fi";
                  Command2 = "@echo Hardware simulation is not enabled for the target SOPC Builder system. Skipping creation of hardware simulation model contents and simulation symbol files. \\(Note: This does not affect the instruction set simulator.\\)";
                  Command3 = "touch $(SIMDIR)/dummy_file";
                  Dependency = "$(ELF)";
                  Target_File = "$(SIMDIR)/dummy_file";
               }
            }
         }
         clockunit = "kHz";
         contents_info = "SIMDIR/epcs_controller_boot_rom.hex 1130817967 SIMDIR/epcs_controller_boot_rom.dat 1130817967 ";
         delayunit = "us";
      }
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/epcs_controller.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
      }
   }
   MODULE jtag_uart_0
   {
      class = "altera_avalon_jtag_uart";
      class_version = "5.11";
      iss_model_name = "altera_avalon_jtag_uart";
      SLAVE avalon_jtag_slave
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Printable_Device = "1";
            Address_Alignment = "native";
            Address_Width = "1";
            Data_Width = "32";
            Has_IRQ = "1";
            Read_Wait_States = "peripheral_controlled";
            Write_Wait_States = "peripheral_controlled";
            JTAG_Hub_Base_Id = "0x04006E";
            JTAG_Hub_Instance_Id = "0";
            Connection_Limit = "1";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "1";
            }
            Base_Address = "0x004810B0";
            Address_Group = "0";
         }
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT rst_n
            {
               type = "reset_n";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_chipselect
            {
               type = "chipselect";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_address
            {
               type = "address";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_read_n
            {
               type = "read_n";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_readdata
            {
               type = "readdata";
               direction = "output";
               width = "32";
               Is_Enabled = "1";
            }
            PORT av_write_n
            {
               type = "write_n";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_writedata
            {
               type = "writedata";
               direction = "input";
               width = "32";
               Is_Enabled = "1";
            }
            PORT av_waitrequest
            {
               type = "waitrequest";
               direction = "output";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_irq
            {
               type = "irq";
               direction = "output";
               width = "1";
               Is_Enabled = "1";
            }
            PORT dataavailable
            {
               Is_Enabled = "1";
               direction = "output";
               type = "dataavailable";
               width = "1";
            }
            PORT readyfordata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readyfordata";
               width = "1";
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Iss_Launch_Telnet = "0";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            Settings_Summary = "<br>Write Depth: 64; Write IRQ Threshold: 8
                <br>Read  Depth: 64; Read  IRQ Threshold: 8";
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         write_depth = "64";
         read_depth = "64";
         write_threshold = "8";
         read_threshold = "8";
         read_char_stream = "";
         showascii = "1";
         read_le = "0";
         write_le = "0";
         altera_show_unreleased_jtag_uart_features = "0";
      }
      SIMULATION 
      {
         Fix_Me_Up = "";
         DISPLAY 
         {
            SIGNAL av_chipselect
            {
               name = "av_chipselect";
            }
            SIGNAL av_address
            {
               name = "av_address";
               radix = "hexadecimal";
            }
            SIGNAL av_read_n
            {
               name = "av_read_n";
            }
            SIGNAL av_readdata
            {
               name = "av_readdata";
               radix = "hexadecimal";
            }
            SIGNAL av_write_n
            {
               name = "av_write_n";
            }
            SIGNAL av_writedata
            {
               name = "av_writedata";
               radix = "hexadecimal";
            }
            SIGNAL av_waitrequest
            {
               name = "av_waitrequest";
            }
            SIGNAL av_irq
            {
               name = "av_irq";
            }
            SIGNAL dataavailable
            {
               name = "dataavailable";
            }
            SIGNAL readyfordata
            {
               name = "readyfordata";
            }
         }
         INTERACTIVE_IN drive
         {
            enable = "0";
            file = "_input_data_stream.dat";
            mutex = "_input_data_mutex.dat";
            log = "_in.log";
            rate = "100";
            signals = "temp,list";
            exe = "nios2-terminal";
         }
         INTERACTIVE_OUT log
         {
            enable = "1";
            exe = "perl -- atail-f.pl";
            file = "_output_stream.dat";
            radix = "ascii";
            signals = "temp,list";
         }
      }
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/jtag_uart_0.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
      }
   }
   MODULE uart_0
   {
      class = "altera_avalon_uart";
      class_version = "5.11";
      iss_model_name = "altera_avalon_uart";
      PORT_WIRING 
      {
         PORT rxd
         {
            direction = "input";
            width = "1";
            Is_Enabled = "1";
            originally_shared = "0";
            is_shared = "0";
         }
         PORT txd
         {
            direction = "output";
            width = "1";
            Is_Enabled = "1";
            originally_shared = "0";
            is_shared = "0";
         }
         PORT cts_n
         {
            direction = "input";
            width = "1";
            Is_Enabled = "0";
         }
         PORT rts_n
         {
            direction = "output";
            width = "1";
            Is_Enabled = "0";
         }
      }
      SLAVE s1
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Printable_Device = "1";
            Address_Alignment = "native";
            Address_Width = "3";
            Data_Width = "16";
            Has_IRQ = "1";
            Read_Wait_States = "1";
            Write_Wait_States = "1";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "2";
            }
            Base_Address = "0x00481000";
            Address_Group = "0";
         }
         PORT_WIRING 
         {
            PORT address
            {
               Is_Enabled = "1";
               direction = "input";
               type = "address";
               width = "3";
            }
            PORT begintransfer
            {
               Is_Enabled = "1";
               direction = "input";
               type = "begintransfer";
               width = "1";
            }
            PORT chipselect
            {
               Is_Enabled = "1";
               direction = "input";
               type = "chipselect";
               width = "1";
            }
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT dataavailable
            {
               Is_Enabled = "1";
               direction = "output";
               type = "dataavailable";
               width = "1";
            }
            PORT irq
            {
               Is_Enabled = "1";
               direction = "output";
               type = "irq";
               width = "1";
            }
            PORT read_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "read_n";
               width = "1";
            }
            PORT readdata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readdata";
               width = "16";
            }
            PORT readyfordata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readyfordata";
               width = "1";
            }
            PORT reset_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset_n";
               width = "1";
            }
            PORT write_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "write_n";
               width = "1";
            }
            PORT writedata
            {
               Is_Enabled = "1";
               direction = "input";
               type = "writedata";
               width = "16";
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Iss_Launch_Telnet = "0";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            Settings_Summary = "8-bit UART with 115200 baud, <br>
                    1 stop bits and N parity";
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL a
            {
               name = "  Bus Interface";
               format = "Divider";
            }
            SIGNAL b
            {
               name = "chipselect";
            }
            SIGNAL c
            {
               name = "address";
               radix = "hexadecimal";
            }
            SIGNAL d
            {
               name = "writedata";
               radix = "hexadecimal";
            }
            SIGNAL e
            {
               name = "readdata";
               radix = "hexadecimal";
            }
            SIGNAL f
            {
               name = "  Internals";
               format = "Divider";
            }
            SIGNAL g
            {
               name = "tx_ready";
            }
            SIGNAL h
            {
               name = "tx_data";
               radix = "ascii";
            }
            SIGNAL i
            {
               name = "rx_char_ready";
            }
            SIGNAL j
            {
               name = "rx_data";
               radix = "ascii";
            }
         }
         INTERACTIVE_OUT log
         {
            enable = "0";
            file = "_log_module.txt";
            radix = "ascii";
            signals = "temp,list";
            exe = "perl -- tail-f.pl";
         }
         INTERACTIVE_IN drive
         {
            enable = "0";
            file = "_input_data_stream.dat";
            mutex = "_input_data_mutex.dat";
            log = "_in.log";
            rate = "100";
            signals = "temp,list";
            exe = "perl -- uart.pl";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         baud = "115200";
         data_bits = "8";
         fixed_baud = "1";
         parity = "N";
         stop_bits = "1";
         use_cts_rts = "0";
         use_eop_register = "0";
         sim_true_baud = "0";
         sim_char_stream = "";
      }
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/uart_0.v";
         Synthesis_Only_Files = "";
      }
   }
   MODULE timer_0
   {
      class = "altera_avalon_timer";
      class_version = "5.11";
      iss_model_name = "altera_avalon_timer";
      SLAVE s1
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Address_Width = "3";
            Data_Width = "16";
            Has_IRQ = "1";
            Read_Wait_States = "1";
            Write_Wait_States = "0";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "3";
            }
            Base_Address = "0x00481020";
            Address_Group = "0";
         }
         PORT_WIRING 
         {
            PORT address
            {
               Is_Enabled = "1";
               direction = "input";
               type = "address";
               width = "3";
            }
            PORT chipselect
            {
               Is_Enabled = "1";
               direction = "input";
               type = "chipselect";
               width = "1";
            }
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT irq
            {
               Is_Enabled = "1";
               direction = "output";
               type = "irq";
               width = "1";
            }
            PORT readdata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readdata";
               width = "16";
            }
            PORT reset_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset_n";
               width = "1";
            }
            PORT write_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "write_n";
               width = "1";
            }
            PORT writedata
            {
               Is_Enabled = "1";
               direction = "input";
               type = "writedata";
               width = "16";
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            Settings_Summary = "Timer with 1 ms timeout period.";
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         always_run = "0";
         fixed_period = "0";
         snapshot = "1";
         period = "1";
         period_units = "ms";
         reset_output = "0";
         timeout_pulse_output = "0";
         mult = "0.001";
      }
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/timer_0.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
      }
   }
   MODULE timer_1
   {
      class = "altera_avalon_timer";
      class_version = "5.11";
      iss_model_name = "altera_avalon_timer";
      SLAVE s1
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Address_Width = "3";
            Data_Width = "16";
            Has_IRQ = "1";
            Read_Wait_States = "1";
            Write_Wait_States = "0";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "4";
            }
            Base_Address = "0x00481040";
            Address_Group = "0";
         }
         PORT_WIRING 
         {
            PORT address
            {
               Is_Enabled = "1";
               direction = "input";
               type = "address";
               width = "3";
            }
            PORT chipselect
            {
               Is_Enabled = "1";
               direction = "input";
               type = "chipselect";
               width = "1";
            }
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT irq
            {
               Is_Enabled = "1";
               direction = "output";
               type = "irq";
               width = "1";
            }
            PORT readdata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readdata";
               width = "16";
            }
            PORT reset_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset_n";
               width = "1";
            }
            PORT write_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "write_n";
               width = "1";
            }
            PORT writedata
            {
               Is_Enabled = "1";
               direction = "input";
               type = "writedata";
               width = "16";
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            Settings_Summary = "Timer with 1 ms timeout period.";
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         always_run = "0";
         fixed_period = "0";
         snapshot = "1";
         period = "1";
         period_units = "ms";
         reset_output = "0";
         timeout_pulse_output = "0";
         mult = "0.001";
      }
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/timer_1.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
      }
   }
   MODULE lcd_16207_0
   {
      class = "altera_avalon_lcd_16207";
      class_version = "5.1";
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/lcd_16207_0.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
         PORT LCD_data
         {
            direction = "inout";
            width = "8";
            Is_Enabled = "1";
            originally_shared = "0";
            is_shared = "0";
            BOARD_COMPONENT altera_nios_dev_board_cyclone_1c20
            {
               component_pin = "J12.7,J12.8,J12.9,J12.10,J12.11,J12.12,J12.13,J12.14";
               pin_assignment = "H14,J14,J17,J18,K15,W18,V18,V19";
            }
            BOARD_COMPONENT de2_board
            {
               component_pin = "U2.7,U2.8,U2.9,U2.10,U2.11,U2.12,U2.13,U2.14";
               pin_assignment = "J1,J2,H1,H2,J4,J3,H4,H3";
            }
            BOARD_COMPONENT altera_nios_dev_board_cyclone_2c35
            {
               component_pin = "J12.7,J12.8,J12.9,J12.10,J12.11,J12.12,J12.13,J12.14";
               pin_assignment = "R19,T19,U20,U21,V26,V25,V24,V23";
            }
         }
         PORT LCD_E
         {
            direction = "output";
            width = "1";
            Is_Enabled = "1";
            originally_shared = "0";
            is_shared = "0";
            BOARD_COMPONENT altera_nios_dev_board_cyclone_1c20
            {
               component_pin = "J12.6";
               pin_assignment = "J20";
            }
            BOARD_COMPONENT de2_board
            {
               component_pin = "U2.6";
               pin_assignment = "K3";
            }
            BOARD_COMPONENT altera_nios_dev_board_cyclone_2c35
            {
               component_pin = "J12.6";
               pin_assignment = "U26";
            }
         }
         PORT LCD_RS
         {
            direction = "output";
            width = "1";
            Is_Enabled = "1";
            originally_shared = "0";
            is_shared = "0";
            BOARD_COMPONENT altera_nios_dev_board_cyclone_1c20
            {
               component_pin = "J12.4";
               pin_assignment = "J15";
            }
            BOARD_COMPONENT de2_board
            {
               component_pin = "U2.4";
               pin_assignment = "K1";
            }
            BOARD_COMPONENT altera_nios_dev_board_cyclone_2c35
            {
               component_pin = "J12.4";
               pin_assignment = "T18";
            }
         }
         PORT LCD_RW
         {
            direction = "output";
            width = "1";
            Is_Enabled = "1";
            originally_shared = "0";
            is_shared = "0";
            BOARD_COMPONENT altera_nios_dev_board_cyclone_1c20
            {
               component_pin = "J12.5";
               pin_assignment = "J19";
            }
            BOARD_COMPONENT altera_nios_dev_board_cyclone_2c35
            {
               component_pin = "J12.5";
               pin_assignment = "T17";
            }
            BOARD_COMPONENT de2_board
            {
               component_pin = "U2.5";
               pin_assignment = "K4";
            }
         }
      }
      SLAVE control_slave
      {
         PORT_WIRING 
         {
            PORT address
            {
               Is_Enabled = "1";
               direction = "input";
               type = "address";
               width = "2";
            }
            PORT begintransfer
            {
               Is_Enabled = "1";
               direction = "input";
               type = "begintransfer";
               width = "1";
            }
            PORT irq
            {
               Is_Enabled = "1";
               direction = "output";
               type = "irq";
               width = "1";
            }
            PORT read
            {
               Is_Enabled = "1";
               direction = "input";
               type = "read";
               width = "1";
            }
            PORT readdata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readdata";
               width = "8";
            }
            PORT write
            {
               Is_Enabled = "1";
               direction = "input";
               type = "write";
               width = "1";
            }
            PORT writedata
            {
               Is_Enabled = "1";
               direction = "input";
               type = "writedata";
               width = "8";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Has_IRQ = "0";
            Is_Printable_Device = "1";
            Address_Width = "2";
            Data_Width = "8";
            Base_Address = "0x00481060";
            Address_Alignment = "native";
            Read_Wait_States = "250ns";
            Write_Wait_States = "250ns";
            Setup_Time = "250ns";
            Hold_Time = "250ns";
            Read_Latency = "0";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Address_Group = "0";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Date_Modified = "";
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         View 
         {
            Is_Collapsed = "1";
            MESSAGES 
            {
            }
         }
         Clock_Source = "clk";
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
      }
   }
   MODULE led_red
   {
      class = "altera_avalon_pio";
      class_version = "5.11";
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/led_red.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "18";
         }
         PORT out_port
         {
            direction = "output";
            Is_Enabled = "1";
            width = "18";
            originally_shared = "0";
            is_shared = "0";
            BOARD_COMPONENT de2_board
            {
               pin_assignment = ",,,,,,,,,,,,,,,,,";
               component_pin = ",,,,,,,,,,,,,,,,,";
            }
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "18";
         }
      }
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT address
            {
               Is_Enabled = "1";
               direction = "input";
               type = "address";
               width = "2";
            }
            PORT chipselect
            {
               Is_Enabled = "1";
               direction = "input";
               type = "chipselect";
               width = "1";
            }
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT reset_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset_n";
               width = "1";
            }
            PORT write_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "write_n";
               width = "1";
            }
            PORT writedata
            {
               Is_Enabled = "1";
               direction = "input";
               type = "writedata";
               width = "18";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Has_IRQ = "0";
            Address_Width = "2";
            Data_Width = "18";
            Base_Address = "0x00481070";
            Address_Alignment = "native";
            Read_Wait_States = "1";
            Write_Wait_States = "0";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Address_Group = "0";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Date_Modified = "";
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            Settings_Summary = " 18-bit PIO using <br>
					
					
					 output pins";
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0x0000";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         edge_type = "NONE";
         irq_type = "NONE";
      }
   }
   MODULE led_green
   {
      class = "altera_avalon_pio";
      class_version = "5.11";
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/led_green.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "0";
            width = "9";
         }
         PORT out_port
         {
            direction = "output";
            Is_Enabled = "1";
            width = "9";
            originally_shared = "0";
            is_shared = "0";
            BOARD_COMPONENT de2_board
            {
               pin_assignment = ",,,,,,,,";
               component_pin = ",,,,,,,,";
            }
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "9";
         }
      }
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT address
            {
               Is_Enabled = "1";
               direction = "input";
               type = "address";
               width = "2";
            }
            PORT chipselect
            {
               Is_Enabled = "1";
               direction = "input";
               type = "chipselect";
               width = "1";
            }
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT reset_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset_n";
               width = "1";
            }
            PORT write_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "write_n";
               width = "1";
            }
            PORT writedata
            {
               Is_Enabled = "1";
               direction = "input";
               type = "writedata";
               width = "9";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Has_IRQ = "0";
            Address_Width = "2";
            Data_Width = "9";
            Base_Address = "0x00481080";
            Address_Alignment = "native";
            Read_Wait_States = "1";
            Write_Wait_States = "0";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Address_Group = "0";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Date_Modified = "";
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            Settings_Summary = " 9-bit PIO using <br>
					
					
					 output pins";
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0x0000";
         has_tri = "0";
         has_out = "1";
         has_in = "0";
         capture = "0";
         edge_type = "NONE";
         irq_type = "NONE";
      }
   }
   MODULE button_pio
   {
      class = "altera_avalon_pio";
      class_version = "5.11";
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/button_pio.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "1";
            width = "4";
            originally_shared = "0";
            is_shared = "0";
         }
         PORT out_port
         {
            direction = "output";
            Is_Enabled = "0";
            width = "4";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "4";
         }
      }
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT address
            {
               Is_Enabled = "1";
               direction = "input";
               type = "address";
               width = "2";
            }
            PORT chipselect
            {
               Is_Enabled = "1";
               direction = "input";
               type = "chipselect";
               width = "1";
            }
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT irq
            {
               Is_Enabled = "1";
               direction = "output";
               type = "irq";
               width = "1";
            }
            PORT readdata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readdata";
               width = "4";
            }
            PORT reset_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset_n";
               width = "1";
            }
            PORT write_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "write_n";
               width = "1";
            }
            PORT writedata
            {
               Is_Enabled = "1";
               direction = "input";
               type = "writedata";
               width = "4";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Has_IRQ = "1";
            Address_Width = "2";
            Data_Width = "4";
            Base_Address = "0x00481090";
            Address_Alignment = "native";
            Read_Wait_States = "1";
            Write_Wait_States = "0";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "5";
            }
            Address_Group = "0";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Date_Modified = "";
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            Settings_Summary = " 4-bit PIO using <br>
					
					 input pins with edge type FALLING and interrupt source EDGE
					";
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0x0000";
         has_tri = "0";
         has_out = "0";
         has_in = "1";
         capture = "1";
         edge_type = "FALLING";
         irq_type = "EDGE";
      }
   }
   MODULE switch_pio
   {
      class = "altera_avalon_pio";
      class_version = "5.11";
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/switch_pio.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
         PORT in_port
         {
            direction = "input";
            Is_Enabled = "1";
            width = "18";
            originally_shared = "0";
            is_shared = "0";
            BOARD_COMPONENT de2_board
            {
               component_pin = ",,,,,,,,,,,,,,,,,";
               pin_assignment = ",,,,,,,,,,,,,,,,,";
            }
            BOARD_COMPONENT untitled
            {
               component_pin = ",,,,,,,,,,,,,,,,,";
               pin_assignment = ",,,,,,,,,,,,,,,,,";
            }
         }
         PORT out_port
         {
            direction = "output";
            Is_Enabled = "0";
            width = "18";
         }
         PORT bidir_port
         {
            direction = "inout";
            Is_Enabled = "0";
            width = "18";
         }
      }
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT address
            {
               Is_Enabled = "1";
               direction = "input";
               type = "address";
               width = "2";
            }
            PORT clk
            {
               Is_Enabled = "1";
               direction = "input";
               type = "clk";
               width = "1";
            }
            PORT readdata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readdata";
               width = "18";
            }
            PORT reset_n
            {
               Is_Enabled = "1";
               direction = "input";
               type = "reset_n";
               width = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Has_IRQ = "0";
            Address_Width = "2";
            Data_Width = "18";
            Base_Address = "0x004810A0";
            Address_Alignment = "native";
            Read_Wait_States = "1";
            Write_Wait_States = "0";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Address_Group = "0";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Date_Modified = "";
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Wire_Test_Bench_Values = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            Settings_Summary = " 18-bit PIO using <br>
					
					 input pins with edge type NONE and interrupt source NONE
					";
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Do_Test_Bench_Wiring = "0";
         Driven_Sim_Value = "0x0000";
         has_tri = "0";
         has_out = "0";
         has_in = "1";
         capture = "0";
         edge_type = "NONE";
         irq_type = "NONE";
      }
   }
   MODULE SEG7_Display
   {
      class = "user_logic_SEG7_LUT_8";
      class_version = "2.0";
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Date_Modified = "--unknown--";
         Clock_Source = "clk";
         View 
         {
            Is_Collapsed = "1";
            MESSAGES 
            {
            }
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
      }
      SLAVE avalonS
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Address_Alignment = "native";
            Address_Width = "0";
            Data_Width = "32";
            Has_IRQ = "0";
            Has_Base_Address = "1";
            Read_Wait_States = "0ns";
            Write_Wait_States = "0ns";
            Setup_Time = "0ns";
            Hold_Time = "0ns";
            Is_Memory_Device = "0";
            Uses_Tri_State_Data_Bus = "0";
            Is_Enabled = "1";
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            Base_Address = "0x004810C0";
            Address_Group = "0";
         }
         PORT_WIRING 
         {
            PORT oSEG0
            {
               width = "7";
               direction = "output";
               type = "export";
            }
            PORT oSEG1
            {
               width = "7";
               direction = "output";
               type = "export";
            }
            PORT oSEG2
            {
               width = "7";
               direction = "output";
               type = "export";
            }
            PORT oSEG3
            {
               width = "7";
               direction = "output";
               type = "export";
            }
            PORT oSEG4
            {
               width = "7";
               direction = "output";
               type = "export";
            }
            PORT oSEG5
            {
               width = "7";
               direction = "output";
               type = "export";
            }
            PORT oSEG6
            {
               width = "7";
               direction = "output";
               type = "export";
            }
            PORT oSEG7
            {
               width = "7";
               direction = "output";
               type = "export";
            }
            PORT iDIG
            {
               width = "32";
               direction = "input";
               type = "writedata";
            }
            PORT iWR
            {
               width = "1";
               direction = "input";
               type = "write";
            }
            PORT iCLK
            {
               width = "1";
               direction = "input";
               type = "clk";
            }
            PORT iRST_N
            {
               width = "1";
               direction = "input";
               type = "reset_n";
            }
         }
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL a
            {
               name = "oSEG0";
               radix = "hexadecimal";
            }
            SIGNAL b
            {
               name = "oSEG1";
               radix = "hexadecimal";
            }
            SIGNAL c
            {
               name = "oSEG2";
               radix = "hexadecimal";
            }
            SIGNAL d
            {
               name = "oSEG3";
               radix = "hexadecimal";
            }
            SIGNAL e
            {
               name = "oSEG4";
               radix = "hexadecimal";
            }
            SIGNAL f
            {
               name = "oSEG5";
               radix = "hexadecimal";
            }
            SIGNAL g
            {
               name = "oSEG6";
               radix = "hexadecimal";
            }
            SIGNAL h
            {
               name = "oSEG7";
               radix = "hexadecimal";
            }
            SIGNAL i
            {
               name = "iDIG";
               radix = "hexadecimal";
            }
            SIGNAL j
            {
               name = "iWR";
            }
            SIGNAL k
            {
               name = "iCLK";
            }
            SIGNAL l
            {
               name = "iRST_N";
            }
         }
      }
      HDL_INFO 
      {
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/SEG7_LUT.v,__PROJECT_DIRECTORY__/SEG7_LUT_8.v, __PROJECT_DIRECTORY__/SEG7_Display.v";
      }
   }
   MODULE DM9000A
   {
      class = "user_logic_DM9000A";
      class_version = "2.0";
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Date_Modified = "--unknown--";
         Clock_Source = "clk";
         View 
         {
            Is_Collapsed = "1";
            MESSAGES 
            {
            }
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
      }
      SLAVE avalonS
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Address_Alignment = "native";
            Address_Width = "1";
            Data_Width = "16";
            Has_IRQ = "1";
            Has_Base_Address = "1";
            Read_Wait_States = "20ns";
            Write_Wait_States = "20ns";
            Setup_Time = "20ns";
            Hold_Time = "20ns";
            Is_Memory_Device = "0";
            Uses_Tri_State_Data_Bus = "0";
            Is_Enabled = "1";
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "8";
            }
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            Base_Address = "0x004810B8";
            Address_Group = "0";
         }
         PORT_WIRING 
         {
            PORT iDATA
            {
               width = "16";
               direction = "input";
               type = "writedata";
            }
            PORT oDATA
            {
               width = "16";
               direction = "output";
               type = "readdata";
            }
            PORT iCMD
            {
               width = "1";
               direction = "input";
               type = "address";
            }
            PORT iRD_N
            {
               width = "1";
               direction = "input";
               type = "read_n";
            }
            PORT iWR_N
            {
               width = "1";
               direction = "input";
               type = "write_n";
            }
            PORT iCS_N
            {
               width = "1";
               direction = "input";
               type = "chipselect_n";
            }
            PORT iRST_N
            {
               width = "1";
               direction = "input";
               type = "reset_n";
            }
            PORT oINT
            {
               width = "1";
               direction = "output";
               type = "irq";
            }
            PORT ENET_DATA
            {
               width = "16";
               direction = "inout";
               type = "export";
            }
            PORT ENET_CMD
            {
               width = "1";
               direction = "output";
               type = "export";
            }
            PORT ENET_RD_N
            {
               width = "1";
               direction = "output";
               type = "export";
            }
            PORT ENET_WR_N
            {
               width = "1";
               direction = "output";
               type = "export";
            }
            PORT ENET_CS_N
            {
               width = "1";
               direction = "output";
               type = "export";
            }
            PORT ENET_RST_N
            {
               width = "1";
               direction = "output";
               type = "export";
            }
            PORT ENET_INT
            {
               width = "1";
               direction = "input";
               type = "export";
            }
         }
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL a
            {
               name = "iDATA";
               radix = "hexadecimal";
            }
            SIGNAL b
            {
               name = "oDATA";
               radix = "hexadecimal";
            }
            SIGNAL c
            {
               name = "iCMD";
            }
            SIGNAL d
            {
               name = "iRD_N";
            }
            SIGNAL e
            {
               name = "iWR_N";
            }
            SIGNAL f
            {
               name = "iCS_N";
            }
            SIGNAL g
            {
               name = "iRST_N";
            }
            SIGNAL h
            {
               name = "oINT";
            }
            SIGNAL i
            {
               name = "ENET_DATA";
               radix = "hexadecimal";
            }
            SIGNAL j
            {
               name = "ENET_CMD";
            }
            SIGNAL k
            {
               name = "ENET_RD_N";
            }
            SIGNAL l
            {
               name = "ENET_WR_N";
            }
            SIGNAL m
            {
               name = "ENET_CS_N";
            }
            SIGNAL n
            {
               name = "ENET_RST_N";
            }
            SIGNAL o
            {
               name = "ENET_INT";
            }
         }
      }
      HDL_INFO 
      {
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/DM9000A_IF.v, __PROJECT_DIRECTORY__/DM9000A.v";
      }
   }
   MODULE sram_0
   {
      class = "user_logic_SRAM_16Bits_512K";
      class_version = "2.0";
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Date_Modified = "--unknown--";
         Clock_Source = "clk";
         View 
         {
            Is_Collapsed = "1";
            MESSAGES 
            {
            }
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
      }
      SLAVE avalonS
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Address_Alignment = "dynamic";
            Address_Width = "18";
            Data_Width = "16";
            Has_IRQ = "0";
            Has_Base_Address = "1";
            Read_Wait_States = "20ns";
            Write_Wait_States = "20ns";
            Setup_Time = "20ns";
            Hold_Time = "20ns";
            Is_Memory_Device = "1";
            Uses_Tri_State_Data_Bus = "0";
            Is_Enabled = "1";
            MASTERED_BY cpu_0/instruction_master
            {
               priority = "1";
            }
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            Base_Address = "0x00400000";
            Address_Group = "0";
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
         }
         PORT_WIRING 
         {
            PORT oDATA
            {
               width = "16";
               direction = "output";
               type = "readdata";
            }
            PORT iDATA
            {
               width = "16";
               direction = "input";
               type = "writedata";
            }
            PORT iADDR
            {
               width = "18";
               direction = "input";
               type = "address";
            }
            PORT iWE_N
            {
               width = "1";
               direction = "input";
               type = "write_n";
            }
            PORT iOE_N
            {
               width = "1";
               direction = "input";
               type = "outputenable_n";
            }
            PORT iCE_N
            {
               width = "1";
               direction = "input";
               type = "chipselect_n";
            }
            PORT iRST_N
            {
               width = "1";
               direction = "input";
               type = "reset_n";
            }
            PORT iUB_N
            {
               width = "1";
               direction = "input";
               type = "byteenable_n";
            }
            PORT iLB_N
            {
               width = "1";
               direction = "input";
               type = "byteenable_n";
            }
            PORT SRAM_DQ
            {
               width = "16";
               direction = "inout";
               type = "export";
            }
            PORT SRAM_ADDR
            {
               width = "18";
               direction = "output";
               type = "export";
            }
            PORT SRAM_UB_N
            {
               width = "1";
               direction = "output";
               type = "export";
            }
            PORT SRAM_LB_N
            {
               width = "1";
               direction = "output";
               type = "export";
            }
            PORT SRAM_WE_N
            {
               width = "1";
               direction = "output";
               type = "export";
            }
            PORT SRAM_CE_N
            {
               width = "1";
               direction = "output";
               type = "export";
            }
            PORT SRAM_OE_N
            {
               width = "1";
               direction = "output";
               type = "export";
            }
         }
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL a
            {
               name = "oDATA";
               radix = "hexadecimal";
            }
            SIGNAL b
            {
               name = "iDATA";
               radix = "hexadecimal";
            }
            SIGNAL c
            {
               name = "iADDR";
               radix = "hexadecimal";
            }
            SIGNAL d
            {
               name = "iWE_N";
            }
            SIGNAL e
            {
               name = "iOE_N";
            }
            SIGNAL f
            {
               name = "iCE_N";
            }
            SIGNAL g
            {
               name = "iRST_N";
            }
            SIGNAL h
            {
               name = "iUB_N";
            }
            SIGNAL i
            {
               name = "iLB_N";
            }
            SIGNAL j
            {
               name = "SRAM_DQ";
               radix = "hexadecimal";
            }
            SIGNAL k
            {
               name = "SRAM_ADDR";
               radix = "hexadecimal";
            }
            SIGNAL l
            {
               name = "SRAM_UB_N";
            }
            SIGNAL m
            {
               name = "SRAM_LB_N";
            }
            SIGNAL n
            {
               name = "SRAM_WE_N";
            }
            SIGNAL o
            {
               name = "SRAM_CE_N";
            }
            SIGNAL p
            {
               name = "SRAM_OE_N";
            }
         }
      }
      HDL_INFO 
      {
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/SRAM_16Bit_512K.v, __PROJECT_DIRECTORY__/sram_0.v";
      }
   }
}
