ADD_USEDW_MSB_BIT=ON
LPM_HINT=MAXIMIZE_SPEED=7,
LPM_NUMWORDS=256
LPM_SHOWAHEAD=ON
LPM_TYPE=dcfifo
LPM_WIDTH=32
LPM_WIDTHU=9
OVERFLOW_CHECKING=ON
RDSYNC_DELAYPIPE=5
UNDERFLOW_CHECKING=ON
USE_EAB=ON
WRITE_ACLR_SYNCH=OFF
WRSYNC_DELAYPIPE=5
DEVICE_FAMILY="Cyclone II"
aclr
data
rdclk
rdreq
wrclk
wrreq
q
rdempty
wrfull
